**List of capacities of Techno Plating B.V.**

|  |  |  |
| --- | --- | --- |
| **Galvanic treatments external** | **Maximum sizes in mm** | **Maximum weight in kg** |
|  |  |  |
| **(Hard) chromeplating:** | Ø900 x 11.000 | 12.500 |
|  | Ø600 x 14.500 | 6500 |
|  |  |  |
| **Nickelplating (watts,galvanic):** | Ø900 x 11.000 | 12.500 |
|  | Ø1200 x 4000 | 6500 |
| **Mechanical treatments outside** | **Maximum sizes in mm** | **Maximum weight in kg** |
|  |  |  |
| **Beltpolishing** | Ø1200 x 10.000 | 12.500 |
|  | Ø700 x 14.500 | 12.000 |
|  |  |  |
| **Stone Grgrinding** | Ø700 x 5000 | 5000 |
|  |  |  |
| **Turning** | Ø600 x 5000 | 10.000 |
|  |  |  |
| **Galvanic treatments internal** | **Maximum sizes in mm** | **Maximum weight in kg** |
|  |  |  |
| **(Hard) chromeplating:** | Ø550 x 7000 | 6500 |
|  |  |  |
|  |  |  |
| **Nickelplating (watts,galvanic):** | Ø1000 x 4000 | 6500 |
|  |  |  |
| **Mechanical treatments internal** | **Maximum sizes in mm** | **Maximum weight in kg** |
|  |  |  |
| **Honing Internal** | Ø550 x 7000 | 6500 |
| **Honing External** | Ø450 x 12.000 | 12.500 |
|  |  |  |
| **Other information** | **Maximum sizes in mm** | **Maximum weight in kg** |
|  |  |  |
| **Shotblasting on almost every requested roughness.** | Ø2500 x 4500 | 10.000 |
|  |  |  |
| **Grinding possibilities till < 0,01 mm.** | Ø450 x 12.000 | 12.500 |